Language-file
二维构架
结构构件
输入文件
汇报文件
标准材料
标准部分
钢筋混凝土设计数据
结构的
静力分析
结构模型
节点
边缘条件
固定支承
可自由活动
支承的硬度
构架要素
开始节点
终止节点
部分
材料
铰链
硬
仅拉伸
仅压缩
用户定义部分
高度
交叉
区域
断面
区域
二阶
平面动量
钢部分
平面
动量
距离
到顶部
到底部
钢梁
厚度
木材部分
宽度
长方形混凝土部分
深度
距离到
顶部钢筋
距离到
底部钢筋
设计
为
梁
柱
混凝土 T-部分
凸缘深度
钢梁宽度
凸缘宽度
距离到
区域中心
部分
材料
弹性的
恒值
硬性的
恒值
膨胀的
系数
膨胀与横伸的
比例
质量的密度
强度
静态承载量
承载量实例
类型
注释
永久的
可变的
偶然的
可弯的
其他
承载量
组合
承载量实例
因子
承载量组合
分散承载量
承载量
方向
距离从
长度
分散
承载的
要素
坡度+偏心距
坡度
偏心距
集中承载量
重力
力矩
移离原位
旋转
温度性负荷
顶部
底部
要素高度
节点承载量
节点
移动量
转动量
结构上的反应
外围
支承反应力
反应力总量
承载力总量
内部重力及动量
承载力组合
无效的元素
普通性
重力
推动性
重力
弯曲性
动量
规定的纵向
推动性阻力
规定的推动性
应力
应力
比例
普通性
弯曲性
强化力
元素移位
局部的
整体的
节点移位
外围
规定的强化力
应力外围
系统全局
元素全局
规定的
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
empty
矩阵移位方法
单元刚度矩阵
单元变换矩阵
应用的单元刚度和单元变换矩阵
局部坐标
全局坐标
刚度系数
一阶分析，忽略扭曲变形
检查分析设置
弹性模
交叉区
惯性动量
构架要素长度
没有铰链
有一个普通铰链
有一个断面铰链
有一个断面铰链和一个弯曲铰链
有一个弯曲铰链
在开始节点
在最后节点
有两个弯曲铰链
计算元素刚度和转换矩阵
固定端重力和动量
索引
元素索引
负荷案例索引
组合件
组合结构平衡方程
组合结构的
刚度矩阵
节点重力/负荷
计算出来的结构移动量
索引表
总索引
简略索引
结构平衡方程
结构移动量的
浓缩矩阵和解法
组合结构的简约矩阵
组合结构的简约节点
逆刚度矩阵
有助于手工计算
计算结构反作用力
固定边缘条件的刚度子矩阵
节点移动引起的反作用力
外部节点负荷
最终的反作用力
计算要素终端重力和动量
节点移动引起的重力和动量
最终的重力和动量
要素终端移动量
改变
符号
要素矩阵
结构平衡方程
结构反作用力
要素终端重力
节点
构架要素
固定边缘条件
自由性阶数
负荷案例
负荷组合
不确定性阶数
用于计算的时间
一阶分析
二阶分析
忽略断面变形
激活自重负荷
一阶分析
二阶分析
忽略断面变形
包括断面变形
漆
表面
表面
Total
质量
工料清单
构架元
构架元
User section
木材部分
Concrete section T
Concrete section rectangle
European 工字梁; Euronorm 19-57
European standard beam; DIN 1025-1
European wide flange beam; Euronorm 53-62
Wide flange column
Wide flange bearing pile
Channel with parallel flanges; DIN 1026-1
European standard channel; DIN 1026-1
European channel with taper flanges; DIN 1026-1
Tee section; EN 10055
Tee cut from I; Euronorm 19-57
Tee cut from HE; Euronorm 19-57
Square hollow section; EN 10210, EN 10219
Rectangular hollow section; EN 10210, EN 10219
Circular hollow section; EN 10210, EN 10219
cold formed
hot formed
British 通用钢梁; BS 4-1
British joist with taper flanges; BS 4-1
British universal column; BS 4-1
British universal bearing pile; BS 4-1
British parallel flange channel; BS 4-1
British channel with taper flanges; BS 4-1
Tee cut from UB; BS 4-1
British T-section; BS 4-1
American wide flange beam; ASTM A6/A6M-02
American standard beam; ASTM A6/A6M-02
American standard channel; ASTM A6/A6M-02
American channel; ASTM A6/A6M-02
Japanese H Section; JIS G 3192
zz-axis
凸缘
Thickness
半径
Radius
of Gyration
重
心 
改变了的形状
元素移动量
轴重力
断面重力
弯曲动量
轴压强
弯曲压强
断面压强
正应力+弯曲应力
系统 + 负载
角度
工程师
Long Stalk Structural Tee
Structural Tee
American wide flange bearing pile; ASTM A6/A6M-02
Beam Matrix
Coefficient of Subgrade
Foundation Stiffness
Elastic Length
Characteristic Length
沉降
土压力
Element Width
弹性地基 Element
合力
拉应力 
Check for validity
抗压应力
positiv
静 平衡
Vertical Stirrups
Minimum Longitudinal Reinforcement
Maximum Longitudinal Reinforcement
Minimum Shear Reinforcement
许可持有者
不能存入版权信息。
你真的想改变许可证设置吗?
英语
德语
南斯拉夫语
选择 可以 后等结果
系统不能处理.检查你的结构模型.
节点移动量大.检查你的结构模型. 
钢材部分
木材部分
Model Column Method
Slenderness ratio
Limiting slenderness ratio
First order eccentricity
Additional eccentricity
Second order eccentricity
Total 偏心距
结构设计 Values
Radius of 
Gyration
Nonslender (short) Column
Slender Column
Effective Length
Error, column is too slender!
Creep effects are neglected
Isolated column without transverse loads
Check for buckling about the second principal axis with reduced section depth!
Model Column
sway
non-sway
braced
unbraced
considered
not considered
An additional check for buckling about the second principal axis is to be considered
横梁 结构设计
柱 结构设计
拉力 Member
Additional checks for the limit states of cracking are to be considered
Checking of span/depth ratio
平板
平板 结构设计
中文
意大利语
language6
language7
雪
温度
支点
Copyright
Release
CSC
Buckling
Curve
Plastic
Section
Modulus
Elastic
Torsion
Constant
Warping
Constant
Total
Surface
Stability
Flexural Buckling
Lateral-Torsional Buckling
Bending moments due to non-centred connections 
and torsional moments due to element loads 
(shear centre) must be separately investigated.
The buckling design is to be checked for applicability.
Lateral-Torsional Buckling is to be checked separately.  
EOF
