Unicode Data File for TwoDFrame.      Copyright(C) Ralf Martin Hansen
---------------------------------------------------------------------

[VERSION]
File version: e.g. 190 = 1.90
208.000000

[SETTINGS]
TwoDFrame: 1 = TRUE, elements underlined, element names, section, material,
node names, hinge size, force size, force dist, force value, distr offset, graph size,
graph with axis, graph is hatched, deflection scale, value precision
1  1  0  0  0  1  0.002000  0.007000  0.000000  1  1  5.000000  1  0  1  1  100.000000  2

[CADDOCSETTINGS]
MinDocSize x z Current Attribute Layer TxtStyle DimStyle LTScale TxtStyleScale
10.000000  7.500000  1  0  0  0  1.000000  1.000000

[CADVIEWSETTINGS]
GCS RCS Grid x z Snap x z SelectDist GripSnap GripSnapDist Extends x z PlotBlackAndWhite
1  1  1  1.000000  1.000000  0  0.100000  0.100000  8.000000  0  1.414000  10.000000  7.500000  1  

[DEVELOPMENT]
Name, N, V, M, dx, dz, dyy, SigAs, TauAsw, Load case, vertDist, horDist, NumOfElements, Names
DEFAULT  1 1 1 0 0 0 0 0 LC01  3.000000 0.500000 0  


[ATTRIBUTES]
LType:	LTScale:	Thickness:	Color:
5
0  1.000000  1  16777215
-1  1.000000  -1  -1
0  1.000000  3  16777215
0  1.000000  2  16777215
0  1.000000  2  16711680

[LAYERS]
Name:	active: locked: Application: Attribute
1
Ebene  1  0  0  0

[TEXTSTYLES]
Name: Height[m]: Width[m]: Angle[deg]: Color: Weight: Italic: Underline: Model Space: Application: Font:
1
Textstil  0.002500  0.000875  0.000000  -1  400  0  0  1  0  Microsoft Sans Serif

[DIMENSIONSTYLES]
Name: Scale: TickSize[m]: TickType: DimLineExt: ExtLineExt: ExtLineOffset: TxtVertPos: AutoTextScale: AutoTextDec: TxtPos:
1
BemStil  1.000000  0.002000  1  0.001500  0.001500  0.005000  0.001500  1.000000  2  0  0

[POINTS]
x[m]:  z[m]:  Mode  Layer:  Attribute:
0

[LINES]
From x[m]:  z[m]:  To x[m]:  z[m]:  Layer:  Attribute:
0

[RECTANGLES]
MidPt x[m]:  z[m]:  Length:  Height:  Angle:  Layer:  Attribute:
0

[POLYLINES]
Num of Pt: From x[m]: z[m]:  To x[m]: z[m]: closed: filled: hidden line: HatchPattern: Layer: Attribute:
0

[GRAPHS]
Start Pt  EndPt Size Hatched Positive Up Distances GraphData  Layer:	Attribute:
0

[CIRCLES]
x[m]:  z[m]: Radius[m]:  Layer:  Attribute:
0

[ARCS]
x[m]:  z[m]: Radius[m]: StartAngle: EndAngle:  Layer: Attribute:
0

[LINEARDIMENSIONS]
Orientation: ExtLineOrigins: DimLineLocation: DimTextLocation: (RotationAngle):  Text: SwitchMeter: TextStyle: DimensionStyle: Layer: Attribute:
0

[TEXT]
x[m]: z[m]: TextStyle: Layer: Attribute: Angle: Contents:
3
0.000000  1.500000  Development  Development  1 0.000000
Vz [N]
0.000000  4.500000  Development  Development  1 0.000000
Myy [Nm]
0.000000  7.500000  Development  Development  1 0.000000
Nx [N]

[PAGESETTINGS]
Margins Left[m]:  Right[m]:  Top[m]:  Bottom[m]:  Header[m]:  Footer[m]  Page in Header: in Footer: Precision:  CSOrigin x[m] y[m]:
Border: Footer: Header: Titleblock Small: Big: Scale: Orientation: PSCombatible: Comp: Eng: Prj: Elem:
0.015000  0.015000  0.020000  0.020000  0.010000  0.010000  0  0  0.000000  0.000000  1  0  0  1  0  5.000000  1  2  0
Ralf Martin Hansen Software








[PROJECT]
Element Description
DEFAULT
DEFAULT

[PROTOCOL]
Protocol System StaticLoads LCase Reac Mom Bdisp Ndisp MinMax  Reac Mom As Stress Bdisp Ndisp
LComb Reac Mom Bdisp Ndisp Ndisp MDMmat CarOverMat ShortReport Precision H4 H5 Text Caption TableHeader
THPos TableData TDPos BorderSize CellSpacing PageBreak Tree Image Sections Debug OutputLanguage ImageWidth
1  1  1  1  1  1  0  0  0  0  0  0  0  0  0  0  0  0  0  0  0  0  0  0  0  0  0  2  8  8  8  8  8  3  8  3  1  1  0  0  1  0  0  0  1  500

[GLOBALS]
snap NumIt CalcWithShearDisp AutoSelfWeight GraficsPlaces kN HoldRotation
 MaxDisp MaxRot CheckDiagonal Eurocode EE RCFixity MinAs
0.005  1  0  0  10  0  1  0.1  0.1  1  1  1  1  1

[NODES]
Name         x[m]:       z[m]:
7
N01  0.000000  0.000000
N02  0.240000  0.000000
N03  0.480000  0.000000
N04  0.720000  0.000000
N05  0.000000  0.180000
N06  0.240000  0.180000
N07  0.480000  0.180000

[SUPPORTS]
Node     stiffness x[kN/m]  z[kN/m]  yy[kN] Angle[rad]
2
N01  -1.000000  -1.000000  0.000000  0.000000
N05  -1.000000  -1.000000  0.000000  0.000000

[MATERIAL]
Material E[kN/m2] (G[kN/m2]) AlphaT[1/k] nue Rho[kg/m3] GammaM0 GammaM1
1
1  S235JRG2(RSt37-2)  210000000.000000  81000000.000000  240.000000  138.560000  0.000012  0.300000  7850.000000  1.100000  1.000000

[SECTIONS]
All types: Type Series Name h[mm]
0: b[mm] Ax[cm2] Avy[cm2] Avz[cm2] Ixx[cm4] Iyy[cm4] Izz[cm4]
1: 
2: b[mm] tw[mm] tf[mm] r[mm] Rotated
3: t[mm]
4(5): (b[mm]) t[mm] ColdFormed (Rotated)
6: b[mm] tw[mm] tf[mm] r[mm] r2[mm] h1[mm] Rotated
10: b[mm]
11: 
20: 
21: 
22: 
1
0  SE  01  3  1000  1.5  500  0.18  0.15  0.15  0.00135  0.00135  0.00135

[BEAMS]
Name N1 N2 Section Mat Hinges M1 M2 Q1 Q2 N1 N2 no_places comp tens truss 2xElasticFound beta 4xOffsets
10
FE01  N01  N02  SE 01  S235JRG2(RSt37-2)  0.00 0.00 1.00 1.00 1.00 1.00 10 0 0 1 0.000000 0.000000 1.000000 0.000000 0.000000 0.000000 0.000000
FE02  N02  N03  SE 01  S235JRG2(RSt37-2)  0.00 0.00 1.00 1.00 1.00 1.00 10 0 0 1 0.000000 0.000000 1.000000 0.000000 0.000000 0.000000 0.000000
FE03  N03  N04  SE 01  S235JRG2(RSt37-2)  0.00 0.00 1.00 1.00 1.00 1.00 10 0 0 1 0.000000 0.000000 1.000000 0.000000 0.000000 0.000000 0.000000
FE04  N05  N06  SE 01  S235JRG2(RSt37-2)  0.00 0.00 1.00 1.00 1.00 1.00 10 0 0 1 0.000000 0.000000 1.000000 0.000000 0.000000 0.000000 0.000000
FE05  N06  N07  SE 01  S235JRG2(RSt37-2)  0.00 0.00 1.00 1.00 1.00 1.00 10 0 0 1 0.000000 0.000000 1.000000 0.000000 0.000000 0.000000 0.000000
FE06  N02  N06  SE 01  S235JRG2(RSt37-2)  0.00 0.00 1.00 1.00 1.00 1.00 10 0 0 1 0.000000 0.000000 1.000000 0.000000 0.000000 0.000000 0.000000
FE07  N03  N07  SE 01  S235JRG2(RSt37-2)  0.00 0.00 1.00 1.00 1.00 1.00 10 0 0 1 0.000000 0.000000 1.000000 0.000000 0.000000 0.000000 0.000000
FE08  N05  N02  SE 01  S235JRG2(RSt37-2)  0.00 0.00 1.00 1.00 1.00 1.00 10 0 0 1 0.000000 0.000000 1.000000 0.000000 0.000000 0.000000 0.000000
FE09  N06  N03  SE 01  S235JRG2(RSt37-2)  0.00 0.00 1.00 1.00 1.00 1.00 10 0 0 1 0.000000 0.000000 1.000000 0.000000 0.000000 0.000000 0.000000
FE010  N07  N04  SE 01  S235JRG2(RSt37-2)  0.00 0.00 1.00 1.00 1.00 1.00 10 0 0 1 0.000000 0.000000 1.000000 0.000000 0.000000 0.000000 0.000000

[LOADCASES]
gammaG, G_sup, G_inf, Q, A, W, O, Ms, Mt, kmod_G, kmod_Q,kmod_S, psi2, Beam Envelopes, Static Equilibrium
Name  LoadType: 1=PL, 2=VL, 3=AL, 4=WL, 5=OTHER  secondorder=1 Comments
1.350000  1.100000  0.900000  1.500000  1.000000  1.500000  1.000000  1.100000  1.300000  0.600000  0.800000  0.900000  0.300000  0  0
1
LC01  1  0


[LOADCOMBINATIONS]
Name  Limit State gammaM kmod NumLoadcase  Loadcase * mult  Comments
0

[DISTRIBUTED_LOADS]
Element lcase distleft[m] distl lleft[kN/m] lright xldleft xldright Direction
0

[IMPERFECTIONS]
Beam loadcase Inclination [rad]  Eccentricity [m]
0

[CONCENTRATED_LOADS]
Beam  loadcase  dist[m]  X[kN]  Z[kN]  YY[kNm]  x[m]  z[m]  yy[rad] local
0

[THERMAL_LOADS]
Beam  loadcase  T_top[K]  T_bottom[K]
0

[NODE_LOADS]
Node  loadcase  X[kN]  Z[kN]  YY[kNm] x[m] z[m] yy[rad] bSettlement
1
N04  LC01  0.000000  -0.030000  0.000000  0.000000  0.000000  0.000000  1




[END]
